Exersise 3.2

Unsable, one LHP pole. Bode-gain-phase-relation does not hold. 1 zero, 3 poles and final phase is 0 degree, should be -180 degree (3-1)\*(-90)

Poles:

1.2076e+01

-1.2187e+01

-2.2218e-01

>> zero(H)

0